CYPRESS GROVE COMMUNITY DEVELOPMENT DISTRICT DRAINAGE CONNECTION PERMIT APPLICATION FORM July 29, 2022

General Information:
Permittee 	
Contact 	
Phone Number 	
Location of the Property:
General Location of the Property:
Section (S) 	
Township (S) 	
Range (S) 	
Area (acres) 	
Drawings (Please provide two sets):
Location Map (8.5” x 11”)
Site Map (8.5” x 11”) locating canals, water bodies, property boundary, on-site lakes/ponds/canals and location of pipe connection
Control Structure Detail
Drainage Calculations (Per South Florida Water Management District Requirements for L-8 Basin)
Water Quality - There are two methods to determine water quality volume. You must use the method that gives you the highest value.
Method 1 - the first 1.0 inch of run-off for the entire site
Method 2 - use 2.5 inches times percentage of pervious area
Allowable (Design) Discharge, 1 inch per day (27 cfs per square mile) for 25-Year, 3-Day rainfall event
Flood Protection
Roads (10-Year, 1-Day rainfall event with discharge)
Perimeter Berm (25-Year, 3-Day rainfall event with discharge)
Buildings (100-Year, 3-Day rainfall event with no discharge)
Engineer Certification required for both drainage calculations and plans
Note: Cypress Grove Community Districts canal stages are maintained for irrigation purposes ranging from 15.5 NGVD to 18.5’ NGVD.