CYPRESS GROVE COMMUNITY DEVELOPMENT DISTRICT DRAINAGE CONNECTION PERMIT APPLICATION FORM
January 23, 2020

General Information:
Permittee 	FPL	
Contact  Matthew Silver
Phone Number  239-222-1061
Location of the Property:
General Location of the Property:

Section (S)
Township (S)

33
42 South

Range (S)   40 East 

Area (acres)

641.8

Drawings (Please provide two sets):
Location Map (8.5” x 11”)
Site Map (8.5” x 11”) locating canals, water bodies, property boundary, on-site lakes/ponds/canals and location of pipe connection
Control Structure Detail
Drainage Calculations (Per South Florida Water Management District Requirements for L-8 Basin)
Water Quality-First 1.5 inches or 3.75 inches times percentage of
impervious, whichever is greater for an impaired waterbody.
Allowable (Design) Discharge, 1 inch per day (27 cfs per square mile) for
25-Year, 3-Day rainfall event
Flood Protection
Roads (10-Year, 1-Day rainfall event with discharge)
Perimeter Berm (25-Year, 3-Day rainfall event with discharge)
Buildings (100-Year, 3-Day rainfall event with no discharge)
Engineer Certification required for both drainage calculations and plans
Note: Cypress Grove Community Districts canal stages are maintained for irrigation purposes ranging from 15.5 NGVD to 18.5’ NGVD.